E . E l s e n H E R A C o o r d . M t g 4 . 9 . 2 0 0 0 H1

E.Elsen Topics ¥ Summary of run ¥ Status of luminosity upgrade ¥ HERA parameters for restart in 2001

E . E l s e n H E R A C o o r d . M t g 4 . 9 . 2 0 0 0

Summary of Current Run

¥ record luminosity (exceeding expectations) ¥ very stable detector operation

¥ 1 pb -1 of extra data with shifted vertex at 70 cm (before and during the shifted vertex program we experienced increased background levels in the lower part of the VLQ detector. Had to be switched off for the trigger).

¥ 12 GeV have been used parasitically to obtained cross

calibration points from beam gas scattering

69.5 pb -1

E . E l s e n H E R A C o o r d . M t g 4 . 9 . 2 0 0 0

Shutdown

Upgrade Work

¥ Beam pipe : Welding procedure has been established.

H1 pipe is being produced at Brush Wellman.

¥ Magnet construction at BNL being helped by

J.Schaffran.

- GG production (required all tested at H1 10.4.2001)

- GO being tested at DESY (req. 8.2.2001 at H1)

¥ CIP construction on schedule (helped by two technicians of DESY).

¥ CST radiation hard APC:

Submitted together with CMS and SLS: Delivery just before Christmas 2000. Bonding January 2001 - tight.

¥ FTD 5 new planar chambers being tested in hall

PETRA SE

¥ BPC production in Dubna scheduled for arrival Nov. 2000

¥ Luminosity Detectors successful test beam calibration runs at CERN

¥ FNC

Test beam calibration runs at CERN

H1 is on schedule for the shutdown which ends with interlock test on 5.6.2001.

E . E l s e n H E R A C o o r d . M t g 4 . 9 . 2 0 0 0

ForwardTracker

Forward Tracker (5 new planar DC) has been assembled in

Daresbury and is now undergoing cosmics tests at DESY.