Chamber current vs beam current

• Significant improvement since early Dec.

• Highest I_e · I_p = 910 mA^2

Extrapolation to higher I_p

• Conditions from 8.–12.12.

extrapolated.

Recent running

• Since 30.10. HERA delivered about 3.6 pb^{−1}.

• H1 on tape: 3.2 pb^{−1} (91%). • 1.4 pb^{−1} with CJC HV on (43%).

Summary and requests

• The background decreased significantly in the last 10 days.

• We would like to increase I_p beyond 40 mA for higher lumi and I_e beyond 28 mA for further vacuum conditioning.

• We propose to postpone the installation of a rest gas analyzer at NR 3.6 m and 6 m • H1 is efficiently taking data with inclusive DIS triggers. The commissioning of the new Forward Trackers is progressing well.

• The VFPS bypass passed the 22 bar pressure test at the manufacturer and arrives at DESY today. The cold test takes place in January.

• The preparation for the CIP repair is expected to be ready by March, despite problems in PCB production quality.