Data Taking: October 2002

Data Taking: November 2002

Data Taking: December 2002

Data Taking: January 2003

Some Statistics

Month Delivered Used I^{max}_e < I_e > I^{max}_e < I_e > DIS Fills Fills injected Fills HERMES ON October 7 7 23 mA 5 mA 20 mA 10 mA 12.9 k November 43 36 33 mA 20 mA 28 mA 15 mA 252.9 k December 17 11 29 mA 16 mA 25 mA 13 mA 97.6 k January 10 8 36 mA 16 mA 26 mA 14 mA 81.9 k

Detector is in good shape to take data

Taken Data

Projected Statistics till 17th of Feb.: 0.85 Mill. DIS << 1.4 Mill. DIS

Loss in Physics Program

assuming no significant polarization before January 2004 switching to unpolarized target and recoil detector end 2004 - start 2005

Requests

No start of shutdown without clear work plans −→ guarantee foreseeable length 4 Month

HERMES shutdown work assuming 8 hour working days, no weekends: 8 - 9 weeks if GA has to be modified: 4 additional weeks

Run non-colliding beams between now and 17th of February average fill: ∼ 12-16 hours −→ ∼ 2 hours (10% - 20%) on setting up collisions −→ weighted with < I_e > effective gain (20% - 40%)

Dump at 10 mA −→ ∼ 4 hours (20% - 30%)

Have hard competition with COMPASS and RHIC coming online now