Actual situation:

• Reasonable background

Target Cell temp. ∼ 90-100^0K (Tope = 80^0K, Tmax < 130^0K);

BLM few triggers below the warning level; Radiation/Particle Fluxes rate < 50 KHz;

Requests before Polarization Studies:

• ∼2 days of stable e-beam for polarimeter tuning I≥10 mA, fill pattern as will be used for studies;

• Operate transverse target magnet during polarization tuning (target calibration)

Requests before Lumi Operations:

• ∼3 fills with scanning e-beam position lumi acceptance calculation; trigger timing tuning; ... additional calibrations;

Pasquale Di Nezza HERA Coordination Meeting, Sep ’03